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	Figure A-1:  PRE-TEST FRONT VIEW
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	Figure A-2:  POST-TEST FRONT VIEW
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	Figure A-3:  PRE-TEST LEFT SIDE VIEW
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	Figure A-4:  POST-TEST LEFT SIDE VIEW
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	Figure A-5:  PRE-TEST RIGHT SIDE VIEW
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	Figure A-6:  POST-TEST RIGHT SIDE VIEW
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	Figure A-7:  PRE-TEST REAR VIEW
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	Figure A-8:  POST-TEST REAR VIEW
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	Figure A-9:  PRE-TEST LEFT FRONT THREE-QUARTER VIEW


	
	

	A-12
	[image: image10.jpg]020307






	8655-F301-03
	

	
	Figure A-10:  POST-TEST LEFT FRONT THREE-QUARTER VIEW
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	Figure A-11:  PRE-TEST RIGHT REAR THREE-QUARTER VIEW


	
	

	A-14
	[image: image12.jpg]020307






	8655-F301-03
	

	
	Figure A-12:  POST-TEST RIGHT REAR THREE-QUARTER VIEW
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	Figure A-13:  PRE-TEST FRONT UNDERBODY VIEW
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	Figure A-14:  POST-TEST FRONT UNDERBODY VIEW
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	Figure A-15:  PRE-TEST REAR UNDERBODY VIEW
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	Figure A-16:  POST-TEST REAR UNDERBODY VIEW
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	Figure A-17:  CERTIFICATION PLACARD
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	Figure A-18:  TIRE PLACARD
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	Figure A-19:  ROLLOVER 90º
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	Figure A-20:  ROLLOVER 180º
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	Figure A-21:  ROLLOVER 270º
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	Figure A-22:  ROLLOVER 360º


