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Figure A-1  Pre-Test Front View of Test Vehicle
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Figure A-2  Post-Test Front View of Test Vehicle
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Figure A-3  Pre-Test Impacted Side View of Test Vehicle
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Figure A-4  Post-Test Impacted Side View of Test Vehicle
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Figure A-5  Pre-Test Rear View of Test Vehicle
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Figure A-6  Post-Test Rear View of Test Vehicle
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Figure A-7  Pre-Test Frontal View of Impactor Face

[image: image8.jpg]§ N—

A GRS A





Figure A-8  Post-Test Frontal View of Impactor Face
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Figure A-9  Pre-Test Left Side View of Impactor Face

[image: image10.jpg]



Figure A-10  Post-Test Left Side View of Impactor Face
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Figure A-11  Pre-Test Right Side View of Impactor Face
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Figure A-12  Post-Test Right Side View of Impactor Face
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Figure A-13  Pre-Test Top View of Impactor Face
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Figure A-14  Post-Test Top View of Impactor Face
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Figure A-15  Pre-Test View of MDB Showing Contact Switches in Place

Intentionally Left Blank
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Figure A-16  Pre-Test Overhead View of MDB Aligned with Vehicle
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Figure A-17  Post-Test Overhead View of Vehicle and MDB
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Figure A-18  Pre-Test Right Occupant Compartment View of Front SID-IIs
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Figure A-19  Post-Test Right Occupant Compartment View of Front SID-IIs
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Figure A-20  Pre-Test Right Occupant Compartment View of Rear SID-IIs
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Figure A-21  Post-Test Right Occupant Compartment View of Rear SID-IIs
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Figure A-22  Pre-Test Left View of Front SID-IIs - View 1
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Figure A-23  Post-Test Left View of Front SID-IIs View
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Figure A-24  Pre-Test Left View of Front SID-IIs - View 2
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Figure A-25  Pre-Test Front View of Front SID-IIs and Door Clearance
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Figure A-26  Post-Test Front View of Front SID-IIs and Door Clearance
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Figure A-27  Pre-Test Left View of Rear SID-IIs
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Figure A-28  Post-Test Left View of Rear SID-IIs
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Figure A-29  Pre-Test Left of Rear SID-IIs
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Figure A-30  Pre-Test Left View of Rear SID-IIs and Door Clearance
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Figure A-31  Post-Test Left View of Rear SID-IIs and Door Clearance
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Figure A-32  Pre-Test Interior of Front Door
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Figure A-33  Post-Test Interior of Front Door Showing SID-IIs Impact Locations
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Figure A-34  Post-Test Front SID-IIs Contact - View 1
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Figure A-35  Post-Test Front SID-IIs Contact - View 2
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Figure A-36  Post-Test Front SID-IIs Contact - View 3
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Figure A-37  Pre-Test Interior of Rear Door
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Figure A-38  Post-Test Interior of Rear Panel Showing SID-IIs Impact Locations
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Figure A-39  Post-Test Rear SID-IIs Contact - View 1
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Figure A-40  Post-Test Rear SID-IIs Contact - View 2
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Figure A-41  Post-Test Rear SID-IIs Contact - View 3
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Figure A-42  Pre-Test Left Side View of MDB with Impactor Face in Position
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Figure A-43  Pre-Test Primary Impact Point View
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Figure A-44  Post-Test Primary Impact Point View
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Figure A-45  Pre-Test Right Side View of MDB with Impactor Face in Position
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Figure A-46  Pre-Test Secondary Impact Point View
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Figure A-47  Post-Test Secondary Impact Point View
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Figure A-48  Post-Test Vehicle Door Deformation Front Angled View
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Figure A-49  Post-Test Vehicle Door Deformation Rear Angled View
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Figure A-50  Vehicle Certification Label View
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Figure A-51  Vehicle Recommended Tire Pressure Label View


A-29
030915-1

