	
	[image: image1.jpg]2144
2004 VW TOUAREG
30 &FWREAR 7102/04

HTSA No. C45800






	A-3
	

	8655-F301-22
	

	
	Figure A-1 PRE-TEST FRONT VIEW
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	Figure A-2 POST-TEST FRONT VIEW
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	Figure A-3 PRE-TEST LEFT SIDE VIEW
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	Figure A-4 POST-TEST LEFT SIDE VIEW
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	Figure A-5 PRE-TEST RIGHT SIDE VIEW
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	Figure A-6 POST-TEST RIGHT SIDE VIEW
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	Figure A-7 PRE-TEST REAR VIEW
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	Figure A-8 POST-TEST REAR VIEW
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	Figure A-9 PRE-TEST LEFT FRONT THREE-QUARTER VIEW
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	Figure A-10 POST-TEST  LEFT FRONT THREE-QUARTER VIEW

	
	[image: image11.jpg]




	A-13
	

	8655-F301-22
	

	
	Figure A-11 PRE-TEST RIGHT REAR THREE-QUARTER VIEW

	
	[image: image12.jpg]




	A-14
	

	8655-F301-22
	

	
	Figure A-12 POST-TEST RIGHT REAR THREE-QUARTER VIEW
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	Figure A-13 PRE-TEST FRONT UNDERBODY VIEW
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	Figure A-14 POST-TEST FRONT UNDERBODY VIEW
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	Figure A-15 PRE-TEST REAR UNDERBODY VIEW
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	Figure A-16 POST-TEST REAR UNDERBODY VIEW
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	Figure A-17 CERTIFICATION PLACARD
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	Figure A-18 TIRE PLACARD
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	Figure A-19 ROLLOVER 90º
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	Figure A-20 ROLLOVER 180º
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	Figure A-21 ROLLOVER 270º
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	Figure A-22 ROLLOVER 360º


