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SECTION 1

PURPOSE OF COMPLIANCE TEST


This 30 mph rear moving barrier impact test is part of the Federal Motor Vehicle Safety Standard (FMVSS) 301 Compliance Test Program conducted for the National Highway Traffic Safety Administration (NHTSA) by Advanced Information Engineering Services under Contract No. DTNH22-01-C-01025.  The purpose of this test was to determine if the subject vehicle, a 2004 Volkswagen Touareg MPV, meets the performance requirements of FMVSS No. 301, "Fuel System Integrity."  This compliance test was conducted using the requirements found in the OVSC Laboratory Test Procedure No. TP-301-03, dated February 28, 2003.

SECTION 2

COMPLIANCE TEST RESULTS SUMMARY


A 2590 kg 2004 Volkswagen Touareg MPV was impacted from the rear by a 1797 kg moving barrier at a velocity of 47.47 kph (29.5 mph).  The test was performed by Advanced Information Engineering Services on July 2, 2004.


The test vehicle was equipped with a 100 liter fuel tank which was filled to 92.4 percent capacity with stoddard fluid prior to impact.  Additional ballast (57  kg) was secured in the vehicle cargo area.  For the purpose of acquiring information for applied research, one instrumented Part 572 E 50th percentile male Anthropomorphic Test Device (ATD) and one instrumented Part 572 E 50th percentile male ATD were placed in the Left Front and Right Rear occupant seating positions and various instruments were added to the test vehicle.  Research data is presented in a separate report.  

The crash event was recorded by eleven high-speed cameras and one real-time camera.  Camera locations and other pertinent camera information are found on pages 3-9 and 3-10 of this report.    Pre- and post-test photographs of the vehicle can be found in Appendix A.


There was no fuel system fluid spillage following the impact or during any portion of the static rollover test.  The average vehicle longitudinal crush was 128 millimeters.  The vehicle appeared to comply with all the requirements of FMVSS No. 301 "Fuel System Integrity."

SECTION 3

COMPLIANCE TEST DATA

DATA SHEET 1

TEST VEHICLE SPECIFICATIONS

	TEST VEHICLE INFORMATION:



	Year/Make/Model/Body Style:
	2004 Volkswagen Touareg MPV

	NHTSA No.:
	C45800
	;       Color:
	Beige
	

	Engine Data:
	6
	Cylinders;
	-
	CID;
	3.2
	Liters;
	-
	cc

	Placement:
	X
	Longitudinal or In-Line;
	-
	Transverse or Lateral

	Transmission Data:
	5
	Speeds;
	-
	Manual;
	X
	Automatic;
	X
	Overdrive

	Final Drive:
	-
	Rear Wheel Drive;
	-
	Front Wheel Drive;
	X
	Four Wheel Drive

	
	Major Options:
	X
	A/C;
	X
	Power Steering;
	X
	Power Brakes

	
	
	X
	Power Windows;
 
	X
	Power Door Locks;
	X
	Tilt Wheel

	Date Received:
	10/29/2003
	;             Odometer Reading
	354
	km

	Selling Dealer:
	McLoughlin Motors Inc.

	& Address:
	Elmer Hill Road
Rome, NY 13440

	
	

	DATA FROM VEHICLE'S CERTIFICATION LABEL:

	
	Vehicle Manufactured by:
	Volkswagen AG Germany

	
	Date of Manufacture: 
	05/03

	
	VIN:
	WVGBC67L64D003224

	
	GVWR:
	2945
	kg;           GAWR-FRONT:
	1415
	kg;         GAWR-REAR:
	1610
	 kg

	DATA FROM VEHICLE'S TIRE LABEL:

	
	Location of Placard on Vehicle:
	Left B-Pillar

	
	Recommended Tire Size:
	P255/60R17 106 H

	*
	Recommended Cold Tire Pressure:                                      FRONT:
	250
	kPa;      REAR:
	300
	kPa

	DATA FROM TIRE SIDEWALL:

	
	Size of Tires on Test Vehicle:
	P255/60R17 106 H
	Manufacturer:  
	Dunlop

	
	Tire Pressure with Maximum Capacity Vehicle Load:        FRONT:
	350
	kPa;      REAR:
	350
	kPa

	
	Type of Spare Tire:
	195/80-17 106P
	

	VEHICLE CAPACITY DATA:

	
	Type of Front Seats:
	-
	Bench;
	X
	Bucket;
	-
	Split Bench

	
	Number of Occupants:
	2
	Front;
	3
	Rear;
	5
	 Total

	
	Vehicle Capacity Weight  (VCW)     =
	631
	kg

	
	No. of Occupants x  68.04 kg            =
	340.2
	kg

	
	Rated Cargo/Luggage Weight  (RCLW) =

	290.8
	kg (136.1 kg maximum)

	*Tire pressure used for test
   
	
	


DATA SHEET 2

PRE-TEST DATA

	WEIGHT OF TEST VEHICLE AS RECEIVED FROM DEALER  (with maximum fluids)= UDW:

	
	Right Front        =
	605.0
	kg
	Right Rear =
	557.0
	kg

	
	Left Front        =
	595.0
	kg.
	Left Rear =
	557.0
	kg

	
	TOTAL FRONT  =
	1200.0
	kg
	TOTAL REAR  =
	1114.0
	kg

	
	TOTAL DELIVERED WEIGHT =
	2314.0
	kg

	
	% of Total  Front of Vehicle Weight  =
	51.9%
	of Total Rear Weight    =
	48.1%
	

	CALCULATION OF VEHICLE'S TARGET TEST WEIGHT:

	
	Total Delivered Weight                                                  =
	2314.0
	kg

	
	Rated Cargo/Luggage Weight (RCLW)                         =
	136.1
	kg (136.1 kg maximum)

	
	Weight of 2 p.572 Dummies, 74.4 kg                            =
	148.8
	kg

	
	TARGET TEST WEIGHT                                             =
	2598.9
	kg

	WEIGHT OF TEST VEHICLE WITH TWO DUMMIES AND 
	127.2
	KG OF CARGO WEIGHT:

	
	Right Front        =
	674.0
	kg
	Right Rear =
	612.0
	kg

	
	Left Front        =
	673.0
	kg
	Left Rear =
	631.0
	kg

	
	TOTAL FRONT  =
	1347.0
	kg
	TOTAL REAR  =
	1243.0
	kg

	
	TOTAL TEST WEIGHT =
	2590.0
	kg

	
	% of Total  Front of Vehicle Weight  =
	52.0%
	of Total Rear Weight    =
	48.0%
	

	*
	Weight of Ballast Secured in Vehicle  =
	57
	kg
	

	
	Type of Ballast:
	Lead shot
	

	
	Method of Securing Ballast:
	Secured to floor

	
	Vehicle Components Removed for Weight Reduction:
	Right front passenger seat

	VEHICLE ATTITUDE (all dimension in millimeters):

	
	AS DELIVERED:
	    RF
	882
	      LF
	888
	       RR
	900
	      LR
	893
	

	
	AS TESTED:
	    RF
	866
	      LF
	862
	       RR
	880
	      LR
	879
	

	
	Vehicle's Wheel Base:
	2850
	mm

	
	Location of Vehicle's C.G.:
	1368
	millimeters rearward of front wheel center.

	FUEL SYSTEM DATA:

	
	Fuel System Capacity From Owner's Manual  =

	100
	liters

	
	Usable Capacity Figure Furnished by COTR =
	100
	liters

	
	Test Volume Range (91 to 94% of Usable Capacity) =
	91
	to
	94
	liters

	
	ACTUAL TEST VOLUME=
	92.4
	 liters  (with entire fuel system filled)


* Ballast weight includes the RCLW, the weight of drained vehicle fluids and the weight of any removed vehicle

   components less the weight of onboard instrumentation, cameras, and hardware.

DATA SHEET 2 (continued) 
PRE-TEST DATA

	FUEL SYSTEM DATA (continued):

	
	Test Fluid Type:
	Stoddard Solution

	
	Test Fluid Specific Gravity:
	0.764

	
	Test Fluid Kinematic Viscosity:
	0.96
	centistokes

	
	Test Fluid Color:
	Orange
	 ("red" is preferred)

	
	Type of Vehicle Fuel Pump:
	Electric

	
	Electric Fuel Pump Operation with Ignition Switch ON and Engine OFF -

	
	Fuel pump operated.

	
	

	
	Details of Fuel System:
	The filler neck is located on the right side of the vehicle above the rear axle;  The fuel

	
	tank is centered ahead of the rear axle saddled over the vehicle drive shaft and exhaust;  The fuel lines are located 

	
	along the right side of the center drive shaft tunnel.

	
	

	
	Comments:
	The rear hatch glass shattered during the event.   The vehicle outboard safety belt pretensioners 

	
	deployed during the event.

	
	

	
	


DATA SHEET 3

MOVING BARRIER DATA

	WEIGHT OF MOVING BARRIER:

	
	Right Front        =
	504.9
	kg
	Right Rear      =
	393.7
	kg.

	
	Left Front          =
	499.9
	kg
	Left Rear         =
	398.3
	kg

	
	TOTAL FRONT  =
	1004.8
	kg
	TOTAL REAR  =
	792.0
	kg

	
	TOTAL BARRIER WEIGHT =
	1796.8
	kg

	MOVING BARRIER DIMENSIONS:

	
	Barrier Face Height:
	1524
	mm

	
	Barrier Face Width:
	1981
	mm

	
	Barrier Face Ground Clearance:
	127
	mm

	
	Tread Width:
	1511
	mm

	
	Wheel Base:
	3048
	mm

	
	Location of C.G.:
	
	X:
	1344
	mm rearward of front wheel center.

	
	
	
	Y:
	0
	mm from longitudinal-vertical plane of symmetry.

	
	
	
	Z:
	414
	mm above ground.

	MOVING BARRIER TIRES:

	
	Manufacturer:
	Dunlop

	
	Model:
	AT Radial Rover

	
	Size:
	P205/75R15

	
	Recommended Max Pressure:
	240
	kPa:

	MOVING BARRIER ABORT SYSTEM:

	
	Type:
	Trailing cable
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DATA SHEET 4
POST TEST DATA
	TYPE OF TEST:

	
	
	Type of Test:
	Rear Barrier
	Impact Angle:

	0º
	

	
	
	Test Date:
	July 2, 2004
	Time:
	11:30
	Temperature:
	21.7
	oC

	
	
	Vehicle NHTSA No.:
	C45800
	VIN:
	WVGBC67L64D003224

	
	
	Required Impact Velocity Range:
	46.51
	to
	48.12
	kph

	BARRIER IMPACT VELOCITY:  (Speed traps within 5 feet of impact plane.)

	
	
	Trap No. 1   =
	47.47
	kph;     Trap No. 2  =
	47.47
	 kph

	
	
	Average Impact Speed   =
	47.47
	kph
	
	
	

	VEHICLE STATIC CRUSH:

	
	
	Vehicle Length:
	

	
	
	
	Pre-Test
	Left =
	4610
	;  C/L  =
	4760
	Right  =
	4610
	

	
	
	
	Post-Test
	Left =
	4450
	;  C/L  =
	4660
	Right  =
	4485
	

	
	
	
	Crush
	Left =
	160
	;  C/L  =
	100
	Right  =
	125
	

	
	
	
	AVERAGE
	=
	128
	millimeters


DATA SHEET 4 (continued)
POST TEST DATA
	TEST VEHICLE NHTSA NO.:
	C45800
	
	  TEST DATE:
	July 2, 2004

	Vehicle Mfgr./Make/Model:
	2004 Volkswagen Touareg MPV     

	Test vehicle fuel tank filled to 91% to 94% of manufacturer's "usable" capacity and with electric fuel pump operating (if it will operate without engine operation).  Part 572 test dummies located at each front designated seating position.



	************************************************************************************************

	TEST  VEHICLE  IMPACT  TYPE:
	-
	 Frontal  (42.28 kph target velocity)

	
	-
	 Oblique (42.28 kph target velocity) with
	-
	o barrier face first

	
	
	 contacting
	-
	 (driver/passenger) side

	
	
	

	
	X
	 Rear Moving Barrier (42.28 kph target velocity)

	
	-
	 Lateral Moving Barrier (32.19 kph target velocity)

	
	
	

	FUEL  SPILLAGE  MEASUREMENT:
	
	
	ACTUAL
	MAX  ALLOWED
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	1.
	From impact until vehicle motion ceases
	
	0
	28 g

	
	2.
	For five minute period after vehicle motion ceases
	
	0
	28 g.

	
	3.
	For next 25 minutes
	
	0
	28 g/min.

	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	SOLVENT  SPILLAGE  DETAILS:
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	None


DATA SHEET 5

STATIC ROLLOVER TEST DATA
	Table 7
FMVSS NO. 301 - STATIC ROLLOVER DATA SHEET

	

	Vehicle:   2004 Volkswagen Touareg MPV
	NHTSA No.: C45800
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	I.
	DETERMINATION OF SOLVENT COLLECTION TIME PERIOD:

	
	

	Rollover Stage
	Rotation Time

(spec. 1 -3 min)
	FMVSS 301 Hold Time
	Total Time
	Next Whole Minute Interval

	0º - 90º
	1
	minutes
	07
	seconds
	5
	minutes
	6
	minutes
	7
	seconds
	7
	minutes

	90º - 180º
	1
	minutes
	09
	seconds
	5
	minutes
	6
	minutes
	9
	seconds
	7
	minutes

	180º-270º
	1
	minutes
	03
	seconds
	5
	minutes
	6
	minutes
	3
	seconds
	7
	minutes

	270º-360º
	1
	minutes
	09
	seconds
	5
	minutes
	6
	minutes
	9
	seconds
	7
	minutes

	
	
	
	
	

	II.
	FMVSS 301 REQUIREMENTS: (Maximum allowable solvent spillage):

	
	
	
	
	

	First 5 minutes from onset of rotation
	6th min.
	7th min.
	8th min. (if required)

	142 g
	28 g
	28 g
	28 g

	
	
	
	

	III.
	ACTUAL TEST VEHICLE SOLVENT SPILLAGE:

	
	
	
	

	Rollover Stage
	First 5 minutes 

from onset of rotation  (g)
	6th min.

(g)
	7th min.

(g)
	8th min. (if required)

(g)

	0º - 90º
	0
	0
	0
	N/A

	90º - 180º
	0
	0
	0
	N/A

	180º-270º
	0
	0
	0
	N/A

	270º-360º
	0
	0
	0
	N/A

	
	 Note:     Record spillage for whole minute intervals only as determined above. 

	
	
	
	
	
	
	
	
	

	IV.
	SOLVENT SPILLAGE LOCATION(S):

	
	
	
	
	
	
	
	
	

	Rollover Stage
	Spillage Location

	0º - 90º
	None

	90º - 180º
	None

	180º-270º
	None

	270º-360º
	None


DATA SHEET 6
HIGH SPEED CAMERA LOCATIONS
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DATA SHEET 6 (continued)
HIGH SPEED CAMERA LOCATIONS
	 NHTSA No. :  C45800

 Vehicle :     2004 Volkswagen Touareg MPV


	CAMERA NO.
	VIEW
	CAMERA POSITIONS (mm)*
	ANGLE** (degrees)
	LENS 

(mm)
	SPEED

(fps)

	
	
	X
	Y
	Z
	
	
	

	1
	Real-Time Camera
	-
	-
	-
	-
	-
	24

	2
	Left Side View
	17953
	2695
	1130
	-1
	35
	1000

	3
	Right Side View
	17355
	1273
	1122
	0
	35
	1005

	4
	Overhead Overall View
	-508
	0
	9804
	-90
	13
	1005

	5
	Overhead Close View
	-508
	0
	9804
	-105
	13
	1000

	6†
	Onboard Driver View
	1027
	2457
	1232
	-3
	8
	1010

	7†
	Onboard Passenger View
	965
	1590
	1275
	-8
	8
	1000

	8
	Vehicle Rear Underbody View
	0
	1223
	-1956
	90
	13
	1000

	9
	Vehicle Mid-Section Underbody View
	0
	2545
	-1956
	90
	13
	1000

	10
	Vehicle Front Underbody View
	0
	3759
	-1956
	90
	13
	1015


* X = film plant to monorail centerline (+ to left of rail) 

   Y = film plane to impact location (+ ahead of impact location)

   Z  = film plane to ground (+ above ground)

**    = referenced to horizontal plane

† Research cameras – X distance is measured to the reference target plane.

Appendix A

PHOTOGRAPHS

LIST OF PHOTOGRAPHS

	Figure
	Photograph Title
	Page  

	
	
	

	A-1
	PRE-TEST FRONT VIEW
	A-3

	A-2
	POST-TEST FRONT VIEW
	A-4

	A-3
	PRE-TEST LEFT SIDE VIEW
	A-5

	A-4
	POST-TEST LEFT SIDE VIEW
	A-6

	A-5
	PRE-TEST RIGHT SIDE VIEW
	A-7

	A-6
	POST-TEST RIGHT SIDE VIEW
	A-8

	A-7
	PRE-TEST REAR VIEW
	A-9

	A-8
	POST-TEST REAR VIEW
	A-10

	A-9
	PRE-TEST LEFT FRONT THREE-QUARTER VIEW
	A-11

	A-10
	POST-TEST LEFT FRONT THREE-QUARTER VIEW
	A-12

	A-11
	PRE-TEST RIGHT REAR THREE-QUARTER VIEW
	A-13

	A-12
	POST-TEST RIGHT REAR THREE-QUARTER VIEW
	A-14

	A-13
	PRE-TEST FRONT UNDERBODY VIEW
	A-15

	A-14
	POST-TEST FRONT UNDERBODY VIEW
	A-16

	A-15
	PRE-TEST REAR UNDERBODY VIEW
	A-17

	A-16
	POST-TEST REAR UNDERBODY VIEW
	A-18

	A-17
	CERTIFICATION PLACARD
	A-19

	A-18
	TIRE PLACARD
	A-20

	A-19
	ROLLOVER 90
	A-21

	A-20
	ROLLOVER 180
	A-22

	A-21
	ROLLOVER 270
	A-23

	A-22
	ROLLOVER 360
	A-24
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