Data format edition number  :1.3
Laboratory name             :KARCO ENGINEERING
Laboratory contact name     :NOVALUE
Laboratory contact phone    :NOVALUE
Laboratory contact fax      :NOVALUE
Laboratory contact email    :NOVALUE
Laboratory test ref. number :MA5100
Customer name               :NHTSA
Customer test ref. number   :06643
Customer project ref. number:DTNH22-06-D-00027
Customer order number       :NOVALUE
Customer cost unit          :NOVALUE
Customer test engineer name :NOVALUE
Customer test engineer phone:NOVALUE
Customer test engineer fax  :NOVALUE
Customer test engineer email:NOVALUE
Title                       :35 MPH NCAP FRONTAL - 2010 LEXUS RX350 AWD 4-DOOR 
Medium No./number of media  :NOVALUE
Timestamp                   :2024-06-17 03:44:47
Type of the test            :VEHICLE INTO BARRIER
Reference temperature       :32
Relative air humidity       :NOVALUE
Date of the test            :2009-04-22
Number of test objects      :2
Comments                    :OBTAIN ATD AND VEHICLE DATA
Comments                    :DATALINK IS NONE, ON-BOARD DAS
Name of test object 1       :LEXUS RX 350 2010
Velocity test object 1      :15.65
Mass test object 1          :2163
Mass curb object 1          :1986
Driver position object 1    :1
Impact side test object 1   :FR
Type of test object 1       :1
Class of test object 1      :UTILITY VEHICLE
Code of test object 1       :NOVALUE
Name of test object 2       :RIGID LOAD CELL BARRIER
Velocity test object 2      :NOVALUE
Mass test object 2          :NOVALUE
Mass curb object 2          :NOVALUE
Driver position object 2    :NOVALUE
Impact side test object 2   :B
Type of test object 2       :NOVALUE
Class of test object 2      :NOVALUE
Code of test object 2       :NOVALUE
