Comments                    :V06963.RST
Comments                    :
Comments                    :DRIVER RESTRAINT #1 INFORMATION ----------
Vehicle Reference Number 1  :1
Occupant Seat Position 1    :1
Restraint Mount 1           :BC
Restraint Type 1            :3PT
Restraint Deployed 1        :DP
Comments                    :LEFT FRONT BUCKLE PRETENSIONER FIRED AT 100 M
Comments                    :SEC.
Comments                    :
Comments                    :DRIVER RESTRAINT #2 INFORMATION ----------
Vehicle Reference Number 2  :1
Occupant Seat Position 2    :1
Restraint Mount 2           :HS
Restraint Type 2            :ABG
Restraint Deployed 2        :DP
Comments                    :LEFT SIDE CURTAIN FIRED AT 100 MSEC.
Comments                    :
Comments                    :PASSENGER RESTRAINT #1 INFORMATION ----------
Vehicle Reference Number 3  :1
Occupant Seat Position 3    :3
Restraint Mount 3           :BC
Restraint Type 3            :3PT
Restraint Deployed 3        :DP
Comments                    :RIGHT FRONT BUCKLE PRETENSIONER  & RETRACTOR 
Comments                    :FIRED AT 100 MSEC.
Comments                    :
Comments                    :PASSENGER RESTRAINT #2 INFORMATION ----------
Vehicle Reference Number 4  :1
Occupant Seat Position 4    :3
Restraint Mount 4           :HS
Restraint Type 4            :ABG
Restraint Deployed 4        :DP
Comments                    :RIGHT SIDE CURTAIN FIRED AT 100 MSEC.
Comments                    :
Comments                    :PASSENGER RESTRAINT #1 INFORMATION ----------
Vehicle Reference Number 5  :1
Occupant Seat Position 5    :4
Restraint Mount 5           :BC
Restraint Type 5            :3PT
Restraint Deployed 5        :DP
Comments                    :LEFT REAR BUCKLE PRETENSIONER FIRED AT 100 MS
Comments                    :EC.
Comments                    :
Comments                    :PASSENGER RESTRAINT #2 INFORMATION ----------
Vehicle Reference Number 6  :1
Occupant Seat Position 6    :4
Restraint Mount 6           :HS
Restraint Type 6            :ABG
Restraint Deployed 6        :DP
Comments                    :LEFT SIDE CURTAIN FIRED AT 100 MSEC.
