Data format edition number  :1.3
Laboratory name             :KARCO ENGINEERING
Laboratory contact name     :NOVALUE
Laboratory contact phone    :NOVALUE
Laboratory contact fax      :NOVALUE
Laboratory contact email    :NOVALUE
Laboratory test ref. number :R20205382
Customer name               :NHTSA
Customer test ref. number   :11361
Customer project ref. number:DTNH22-14-D-00360
Customer order number       :NOVALUE
Customer cost unit          :NOVALUE
Customer test engineer name :NOVALUE
Customer test engineer phone:NOVALUE
Customer test engineer fax  :NOVALUE
Customer test engineer email:NOVALUE
Title                       :RESEARCH AND DEVELOPMENT FULL FRONTAL RIGID RIGID 
Medium No./number of media  :NOVALUE
Timestamp                   :2025-11-10 07:25:18
Type of the test            :VEHICLE INTO BARRIER
Reference temperature       :19
Relative air humidity       :NOVALUE
Date of the test            :2021-01-08
Number of test objects      :2
Comments                    :TO GENERATE30° FRONTAL RIGID BARRIER IMPACT P
Comments                    :ERFORMANCE INFORMATION
Comments                    :FULL FRONTAL RIGID BARRIER - R20205382 -2020 
Comments                    :HONDA ACCORD
Name of test object 1       :HONDA ACCORD 2020
Velocity test object 1      :10.93
Mass test object 1          :1640
Mass curb object 1          :0
Driver position object 1    :1
Impact side test object 1   :FR
Type of test object 1       :1
Class of test object 1      :FOUR DOOR SEDAN
Code of test object 1       :NOVALUE
Name of test object 2       :RIGID FLAT ANGLED BARRIER
Velocity test object 2      :NOVALUE
Mass test object 2          :NOVALUE
Mass curb object 2          :NOVALUE
Driver position object 2    :NOVALUE
Impact side test object 2   :B
Type of test object 2       :NOVALUE
Class of test object 2      :NOVALUE
Code of test object 2       :NOVALUE
